
FOR IMMEDIATE RELEASE


Oliver Machinery's 6" Jointers Get an Update


------------

RENTON, WA, December 17, 2025 - Our 4225 6" Parallelogram Jointer includes an updated design with relocated power switch and increased horsepower.

The Oliver 4225.215 8" jointer is an excellent choice for those looking for additional cutting capacity. Our freshened up 8" Jointer includes an updated design with relocated power switch and increased horsepower. Equipped with Oliver's true HCX Helical Cutterhead (not a linear spiral design) using 4-sided carbide inserts, it provides excellent cut quality and precision. This jointer has plenty of power, Oliver's famous build quality and is a stand-out in the 6" jointer class.

• Extra-long precision ground tables provide a stable work surface.    

• Parallelogram design provides smooth accurate cuts.    

• Cast iron frame offers stable table support.    

• Fully enclosed cabinet with 4" port for superior dust management.    

• Built-in mobile base with lockable wheels.    

• Cabinet includes push pad storage.    

• Oliver HCX Helical cutterheads with premium carbide inserts.    

• 4-sided cutting inserts are indexed and easy to replace.    

• Lever controlled infeed and outfeed table adjustment allows quick set-up.    

• Long precision ground fence tilts up to 135° with positive stops at 45° and 90°.    

• Easy to read depth of cut gauge.    

• Large, lockable pedestal mounted paddle on/off switch for added safety.    

• Powerful TEFC 1.5HP single-phase motor.    

• Poly V-belt drive efficiently delivers power to the cutter head.    

• CSA Listed.

This machine replaces our 4225.201, it adds the power switch to a perch and increases horsepower from 1HP to 1.5HP. 

The updated SKU is 4225.215 for ordering. In stock and available to ship.


Media Contact: 

Gregg Healy

Phone: 253 867-0334 x111

press@olivermachinery.net